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Certificate of Conformity

 APRON PE 140 X 78 CM   
113-8279

CHARACTERISTICS:

Polyethylene (PE) film, commonly called PE, is made from a mixture of 65% Low Density Polyethylene (LDPE) and 35% Light Low Density Polyethylene (LLDPE). Poly-latex film is very lightweight and is a complex hydrocarbon chain. It is practically impervious; hence it is excellent for containing moisture and dirt. It also repels moisture and oil. PE is non-toxic and odourless. PE has excellent resistance to chemical corrosion and its physical properties and not affected by either chemical or solvents. Since it is a form of plastic material, it possesses excellent strength and it can be easily sealed. It is heavily textured for better grip.

PHYSICAL PROPERTIES

Length (L)					140cm +/- 1cm

Width (W)					78cm +/- 1cm

Wall Thickness					0.02mm +/- 0.001mm

[bookmark: _GoBack]Weight						17 g +/- 5%

Tensile Strength					>40 kg/m2 

Elongation 					100-250%

Colour 						White

PACKING:

100pcs/bag, 10bags/carton case

QUALITY ASSURANCE CRITERIA:

Aprons are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Broken elastic band				4.	Holes/tears in fabric material 
2.	Irregular material					5.	Physical dimensions non-compliance
3.	Dirty						6. 	Not clean
							

Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: Feb 2020




VWR International bvba/sprl, Researchpark Haasrode 2020, Geldenaaksebaan 464, 3001 Leuven, Belgium 
http://www.vwr.com
 
 Version: 3.0
image1.png
VWRE

We Enable Science

uwesa 2




