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VISITORCOAT PP SNAP ELAST.WRIST WH S 
122062

CHARACTERISTICS:

· The visitor coat is made of 35 gsm Polypropylene, no pockets, with 5 snaps in front, with collar, no elastic on wrist.
· Comply with European Commission Directive 1935/2004/EC, Regulation (EU) No.10/2011, Regulation (EU) No. 1416/2016 and Regulation (EU) No. 752/2017.


PHYSICAL PROPERTIES

Material	35gsm SPP 

Color 					White

Dimension				Length 106cm±2cm
[bookmark: OLE_LINK5][bookmark: OLE_LINK6]					Width 64cm±1cm
					Sleeve length 71cm±1cm
					Wrist width 16cm±0.5cm

PACKING:

1pcs/bag, 50bags/case

QUALITY ASSURANCE CRITERIA:

Visitor coats are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Stain and foreign material				4.	Odor
2.	Color variation					5.	Holes or tears
3.	Damage						6.	Physical dimensions non-compliance


Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: November 2015




VWR International bvba/sprl, Researchpark Haasrode 2020, Geldenaaksebaan 464, 3001 Leuven, Belgium 
http://www.vwr.com
 
 Version: 3.0
image1.png
VWRE

We Enable Science

uwesa 2




