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BOUFFANT CAP CLIP GREEN 50 CM - BOX 
113-8249

CHARACTERISTICS:

Bouffant clip caps, also called head covers, are made of 12 grams/m2 by weight, non-woven polypropylene material, commonly used in a clean environment. Bouffant clip caps are manufactured in a stringent clean environment. Colour green.

PHYSICAL PROPERTIES

Material					Non-woven Polypropylene 12grams white
Elastic					latex free

Size					50 cm 

Stretch Length				50 cm +/- 1 cm

Material Thickness			2.0 mils +/- 0.2 mils

[bookmark: _GoBack]Colour					green

Tensile Strength				MD > 16N/5cm;		CD > 10N/5cm

Ultimate Elongation			>30 %

PACKING:

250pcs/ box – 4 boxes/case

QUALITY ASSURANCE CRITERIA:

Bouffant clip caps are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Broken elastic band				4.	Holes/tears in fabric material 
2.	Irregular SPP material				5.	Physical dimensions non-compliance
3.	Dirty						6. 	Not clean
							

Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: Feb 2020
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