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MOBCAP PP RD 52CM
122032

CHARACTERISTICS:

· The mop cap is made of 10 gsm SPP, red with latex free elastic.
· Comply with European Commission Directive 1935/2004/EC, Regulation (EU) No.10/2011, Regulation (EU) No. 1416/2016 and Regulation (EU) No. 752/2017.


PHYSICAL PROPERTIES

Material	10gsm SPP 

Color 					Red

Dimension				Length 52cm±1cm

Elastic band				Latex free


PACKING:

100pcs/bag, 10bags/case

QUALITY ASSURANCE CRITERIA:

Mop caps are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Stain and foreign material				4.	Odor
2.	Color variation					5.	Holes or tears
3.	Damage						6.	Physical dimensions non-compliance


Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: July 2019
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