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Technical Datasheet

SHOECOVER CPE 100µ ANTI-SLIP WH 15X41 
GUNA121354

CHARACTERISTICS:

· [bookmark: _GoBack]The shoe cover is made of 100µm CPE film, anti-slip, white color with elastic at opening.
· Comply with European Commission Directive 1935/2004/EC, Regulation (EU) No.10/2011, Regulation (EU) No. 1416/2016 and Regulation (EU) No. 752/2017.


PHYSICAL PROPERTIES

Material	100µm CPE film 

Color 					White

Dimension				Length 41cm±1cm
[bookmark: OLE_LINK5][bookmark: OLE_LINK6]					Height 15cm±1cm

Weight					13g/pc


PACKING:

5pcs/roll, 10rolls/bag, 10bags/case

QUALITY ASSURANCE CRITERIA:

Shoe covers are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Stain and foreign material				4.	Odor
2.	Color variation					5.	Holes or tears
3.	Damage						6.	Physical dimensions non-compliance


Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: July 2019
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