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Certificate of Conformity

 VWR Coverall, SPP50g, antistatic, white, with hood, 
zip down, elastic cuffs at ankles and waist, serged seam

INTENDED USE

	Food & pharmaceutical industry, lab & research



GENERAL SPECIFICATION

	Item
	Standard

	Material
	50gsm SPP Antistatic

	Color
	White

	Elastic
	Latex free, 4mm width, white

	Zip
	Nylon

	Surface Resistance
	<1010 ohm



MATERIAL SPECIFICATION

50gsm SPP
	Item
	Test method
	average value standard

	
	
	average value
	tolerance for average value

	Weight(g/m2)
	GB/T4669-1995
	50.00
	+/-4

	Break Tensile propertities
	MD
	GB/T3923.1-1997
	Break Tensile propertities

	
	CD
	GB/T3923.1-1997
	>45N/5cm

	Elongation rate(%)
	MD
	GB/T3923.1-1997
	Elongation rate(%)

	
	CD
	GB/T3923.1-1997
	>30%





DIMENSION
[image: ]
	Item
	Unit
	Specification
	Tolerance

	
	
	113-8305
	113-8306
	113-8307
	113-8308
	113-8309
	113-8310
	

	
	
	M
	L
	XL
	XXL
	XXXL
	XXXXL
	

	A) Chest
	cm
	61
	63
	68
	72
	75
	79
	±2.0

	[bookmark: _GoBack]B) Sleeve Outseam
	cm
	87
	91
	93
	94
	96
	100
	±2.0

	C) Body Length
	cm
	87
	88
	95
	97
	102
	105
	±2.0

	D) Inseam
	cm
	77
	80
	82
	80
	85
	87
	±2.0

	E) Zipper
	cm
	70
	70
	80
	80
	85
	85
	±2.0

	[bookmark: _Hlk349144355]F) Wrist Relaxed
	cm
	8
	8
	8
	9
	9
	9
	±1.0

	G) Ankle Relaxed
	cm
	12
	12
	12
	13
	13
	13
	±1.0

	H) Full Length
	cm
	160
	163
	170
	172
	180
	187
	±2.0



PACKAGE

	Package/Quantity
	1pcs/PE bag, 50pcs/Case

	Best storage Conditions
	10° - 30°C

	
	40% - 75% humidity

	
	dry

	Shelf Life
	5 years 

	Country of Origin
	China





QUALITY ASSURANCE CRITERIA:

Coveralls are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Broken elastic band				4.	Holes/tears in fabric material 
2.	Irregular SPP material				5.	Physical dimensions non-compliance
3.	Dirty						6. 	Not clean
							

Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: Feb 2020
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