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SLEEVE WHITE WATERPROOF 40X20CM 
113-8255

CHARACTERISTICS:

SPP coated sleeves are made of 24grams/m2 by weight, PE film coated 24 grams/m2 by weight, non-woven polypropylene material, and available in white colour. SPP coated PE sleeves are manufactured, vacuum-sealed bagged in a stringent clean environment.

PHYSICAL PROPERTIES

Material					Non-woven Polypropylene coated polyethylene 48g white
					With welded elastic cuffs

Size					Large

Length					40cm +/- 1.5cm

Height					20cm +/- 2.5cm

[bookmark: _GoBack]Colour					white

PACKING:

10pcs/bundle, 10bundles/sealed bag, 10bags/case

QUALITY ASSURANCE CRITERIA:

Sleeves are guaranteed to meet 4.0 AQL level II sampling plan per MIL-std-150E for the following defect criteria:

1.	Broken elastic band				4.	Holes/tears in fabric material 
2.	Irregular SPP material				5.	Physical dimensions non-compliance
3.	Dirty						6. 	Not clean
							

Disclaimer: VWR wants to state that this declaration will not discharge the user from his obligation to ensure the product is suitable for the intended use. -  If there is any doubt ask us.

Date of issue: Feb 2020
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