	OPTICAL TUBE INFO:
	

	Optical Design
	Refractor

	Aperture
	80mm (3.1")

	Focal Length
	900mm (35.43")

	Focal Ratio
	f/11

	Focal Length of Eyepiece 1
	25mm (0.98")

	Magnification of Eyepiece 1
	36x

	Focal Length of Eyepiece 2
	10mm (0.39")

	Magnification of Eyepiece 2
	90x

	Barlow Lens
	2x (1.25")

	Finderscope
	StarPointer™ red dot finderscope

	Star Diagonal
	Erect image 90° (1.25")

	Optical Tube
	Aluminum

	Highest Useful Magnification
	189x

	Lowest Useful Magnification
	11x

	Limiting Stellar Magnitude
	12

	Resolution (Rayleigh)
	1.74 arc seconds

	Resolution (Dawes)
	1.45 arc seconds

	Light Gathering Power (Compared to human eye)
	131x

	Optical Coatings
	Fully-Coated glass optics

	Optical Tube Length
	965mm (38")

	Optical Tube Diameter
	90mm (3.54")

	Optical Tube Weight
	5.4 lbs (2.45 kg)

	Dovetail
	None

	MOUNT INFO:
	

	Mount Type
	Manual Alt-Azimuth

	Height adjustment range (includes mount and tripod)
	Aluminum, 1320.8mm (52") max height

	Tripod Leg Diameter
	31.75mm (1.25") steel

	Accessory Tray
	Yes

	Tripod Weight
	3.8 lbs (1.72 kg)

	Slew Speeds
	Manual

	GPS
	Uses phone's GPS

	Dovetail Compatibility
	CG-5 Dovetail bar

	Power Requirements
	None (Recommend PowerTank Glow to keep phone charged while using app)

	Alignment Procedures
	Use StarSense Explorer app

	Software
	StarSense Explorer app | SkyPortal app | Celestron Starry Night Basic Edition Software

	Total Kit Weight
	9.2 lbs (4.17 kg)

	Included Items
	Telescope tube | Mount/tripod (preassembled) | 25mm & 10mm eyepieces | Erect image diagonal | 2x Barlow lens | StarPointer&trade finderscope | Accessory tray | StarSense Explorer phone dock



